SEED BALLS FALL ON THE TRAY

IR SENSOR DETECTS PREPARED SEED BALLS

JET NOZZLE SPRAYS WATER

WATER CONTAINER SENDS WATER VIA TUBE

BARREL STARTS ROTATING

DC MOTOR ON

BLUE LED GLOWS

IR SENSOR DETECTS PRESENCE OF MATERIALS